{"text_format":"1","workbook":"xlsx","n_sheets":5,"sheets":["Dashboard","Data In","Data Out","Settings","Manifest"],"not_rendered":{"charts":2,"images":0,"macros":0,"external_links":0,"defined_names":9,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900"}

{"sheet":"Dashboard","index":0,"n_rows":24,"n_cols":27,"rows_kept":24,"cut":false,"hidden":false,"merged":[[6,1,10,1],[11,1,23,1],[1,1,3,18],[1,19,3,25],[1,26,3,31]]}
[]
[null,"SPECTROSCOPY DASHBOARD",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Select Item →",null,null,null,null,null,null,"Known A"]
[]
[]
[]
[null,null,"Wavelength","Average Intensity"]
[null,"INFRARED","410nm",{"$f":"AVERAGE(TBL_HST[CH1])","v":{"$error":"#DIV/0!"}}]
[null,null,"435nm",{"$f":"AVERAGE(TBL_HST[CH2])","v":{"$error":"#DIV/0!"}}]
[null,null,"460nm",{"$f":"AVERAGE(TBL_HST[CH3])","v":{"$error":"#DIV/0!"}}]
[null,null,"485nm",{"$f":"AVERAGE(TBL_HST[CH4])","v":{"$error":"#DIV/0!"}}]
[null,null,"510nm",{"$f":"AVERAGE(TBL_HST[CH5])","v":{"$error":"#DIV/0!"}}]
[null,"VISIBLE","535nm",{"$f":"AVERAGE(TBL_HST[CH6])","v":{"$error":"#DIV/0!"}}]
[null,null,"560nm",{"$f":"AVERAGE(TBL_HST[CH7])","v":{"$error":"#DIV/0!"}}]
[null,null,"585nm",{"$f":"AVERAGE(TBL_HST[CH8])","v":{"$error":"#DIV/0!"}}]
[null,null,"610nm",{"$f":"AVERAGE(TBL_HST[CH8])","v":{"$error":"#DIV/0!"}}]
[null,null,"645nm",{"$f":"AVERAGE(TBL_HST[CH10])","v":{"$error":"#DIV/0!"}}]
[null,null,"680nm",{"$f":"AVERAGE(TBL_HST[CH11])","v":{"$error":"#DIV/0!"}}]
[null,null,"705nm",{"$f":"AVERAGE(TBL_HST[CH12])","v":{"$error":"#DIV/0!"}}]
[null,null,"730nm",{"$f":"AVERAGE(TBL_HST[CH13])","v":{"$error":"#DIV/0!"}}]
[null,null,"760nm",{"$f":"AVERAGE(TBL_HST[CH14])","v":{"$error":"#DIV/0!"}}]
[null,null,"810nm",{"$f":"AVERAGE(TBL_HST[CH15])","v":{"$error":"#DIV/0!"}}]
[null,null,"860nm",{"$f":"AVERAGE(TBL_HST[CH16])","v":{"$error":"#DIV/0!"}}]
[null,null,"900nm",{"$f":"AVERAGE(TBL_HST[CH17])","v":{"$error":"#DIV/0!"}}]
[null,null,"940nm",{"$f":"AVERAGE(TBL_HST[CH18])","v":{"$error":"#DIV/0!"}}]

{"sheet":"Data In","index":1,"n_rows":7,"n_cols":19,"rows_kept":7,"cut":false,"hidden":false,"merged":[[5,0,5,18],[0,0,0,9],[1,0,1,9],[2,0,2,18]]}
["Data In (From Arduino Uno (COM6))"]
["Data coming from the current data source will appear below as it is received."]
["Current Data"]
["TIME","CH1","CH2","CH3","CH4","CH5","CH6","CH7","CH8","CH9","CH10","CH11","CH12","CH13","CH14","CH15","CH16","CH17","CH18"]
[]
["Historical Data"]
["TIME","CH1","CH2","CH3","CH4","CH5","CH6","CH7","CH8","CH9","CH10","CH11","CH12","CH13","CH14","CH15","CH16","CH17","CH18"]

{"sheet":"Data Out","index":2,"n_rows":5,"n_cols":18,"rows_kept":5,"cut":false,"hidden":false,"merged":[[0,0,0,7],[1,0,1,7]]}
["Data Out (To Device)"]
["Data entered into the channels below will be sent to the currently connected device as a comma-delimited string."]
[]
["CH1","CH2","CH3","CH4","CH5","CH6","CH7","CH8","CH9","CH10","CH11","CH12","CH13","CH14","CH15","CH16","CH17","CH18"]
["GO"]

{"sheet":"Settings","index":3,"n_rows":20,"n_cols":8,"rows_kept":20,"cut":false,"hidden":false,"merged":[[10,0,11,3],[0,0,0,3],[2,0,3,3],[2,5,3,10]]}
["Workbook Settings"]
[]
["Settings below will affect how data is read into the current workbook from data sources. Clear a field's contents to revert to its default setting. Before streaming data, be sure that \"Data channels\" is set to 18!",null,null,null,null,"Type the name and formulas of the substances you plan to use.  See suggestions listed below. WARNING: Deleting the Prefilled \"Unknowns\" will eliminate them from the drop-down menu."]
[]
[]
["Data interval (ms)",null,null,null,null,"Sample Substance A",null,"Known A"]
["Data rows",100,null,null,null,"Sample Substance B",null,"Known B"]
["Data channels",18,null,null,null,"Sample Substance C",null,"Known C"]
["Data orientation","Newest first",null,null,null,null,null,"Unknown - A"]
[null,null,null,null,null,null,null,"Unknown - B"]
["WARNING: Changing settings may result in the loss of content and/or custom formatting in the Data In and Data Out worksheets. Always save before changing values.",null,null,null,null,null,null,"Unknown - C"]
[]
[null,null,null,null,null,"Table Salt (NaCl)",null,"Pencil Lead/Graphite (C)"]
[null,null,null,null,null,"Baking Soda (NaHCO3)",null,"Play Sand (SiO2)"]
[null,null,null,null,null,"Potassium Nitrate (KNO3)",null,"Hydrofluoric Acid (HF)"]
[null,null,null,null,null,"Vinegar/Acetic Acid (CH3COOH)",null,"Phosphoric Acid (H3PO4)"]
[null,null,null,null,null,"Table Sugar/Sucrose (C12H22O12)",null,"Chalk/Calcium Carbonate (CaCO3)"]
[null,null,null,null,null,"Aluminum Foil (Al)",null,"Iron Filings (Fe)"]
[null,null,null,null,null,"Epsom Salt (MgSO4)",null,"Magnesium Ribbon (Mg)"]
[null,null,null,null,null,"Cornstarch (C6H10O5)",null,"Vegetable Oil (C18H34O2)"]

{"sheet":"Manifest","index":4,"n_rows":23,"n_cols":12,"rows_kept":23,"cut":false,"hidden":false,"merged":[[3,8,3,9],[4,8,4,9],[5,8,5,9],[7,8,7,9],[0,0,0,6],[1,0,1,6],[3,1,3,6],[4,1,22,1],[2,1,2,7]]}
["Arduino Uno",null,null,null,null,null,null,null,null,null,null,"{\"Channels\":[{\"Description\":null,\"Id\":null,\"IsGhost\":false,\"Name\":null,\"Status\":\"Active\",\"SubChannels\":[{\"Description\":null,\"Id\":\"CH1\",\"IsGhost\":false,\"Name\":\"CH1\",\"Status\":\"Active\",\"SubChannels\":[],\"UnitOfMeasure\":null},{\"Description\":null,\"Id\":\"CH2\",\"IsGhost\":false,\"Name\":\"CH2\",\"Status\":\"Active\",\"SubChannels\":[],\"UnitOfMeasure\":null},{\"Description\":null,\"Id\":\"CH3\",\"IsGhost\":false,\"Name\":\"CH3\",\"Status\":\"Active\",\"SubChannels\":[],\"UnitOfMeasure\":null},{\"Description\":null,\"Id\":\"CH4\",\"IsGhost\":false,\"Name\":\"CH4\",\"Status\":\"Active\",\"SubChannels\":[],\"UnitOfMeasure\":null},{\"Description\":null,\"Id\":\"CH5\",\"IsGhost\":false,\"Name\":\"CH5\",\"Status\":\"Active\",\"SubChannels\":[],\"UnitOfMeasure\":null},{\"Description\":null,\"Id\":\"CH6\",\"IsGhost\":false,\"Name\":\"CH6\",\"Status\":\"Active\",\"SubChannels\":[],\"UnitOfMeasure\":null},{\"Description\":null,\"Id\":\"CH7\",\"IsGhost\":false,\"Name\":\"CH7\",\"Status\":\"Active\",\"SubChannels\":[],\"UnitOfMeasure\":null},{\"Description\":null,\"Id\":\"CH8\",\"IsGhost\":false,\"Name\":\"CH8\",\"Status\":\"Active\",\"SubChannels\":[],\"UnitOfMeasure\":null},{\"Description\":null,\"Id\":\"CH9\",\"IsGhost\":false,\"Name\":\"CH9\",\"Status\":\"Active\",\"SubChannels\":[],\"UnitOfMeasure\":null},{\"Description\":null,\"Id\":\"CH10\",\"IsGhost\":false,\"Name\":\"CH10\",\"Status\":\"Active\",\"SubChannels\":[],\"UnitOfMeasure\":null},{\"Description\":null,\"Id\":\"CH11\",\"IsGhost\":false,\"Name\":\"CH11\",\"Status\":\"Active\",\"SubChannels\":[],\"UnitOfMeasure\":null},{\"Description\":null,\"Id\":\"CH12\",\"IsGhost\":false,\"Name\":\"CH12\",\"Status\":\"Active\",\"SubChannels\":[],\"UnitOfMeasure\":null},{\"Description\":null,\"Id\":\"CH13\",\"IsGhost\":false,\"Name\":\"CH13\",\"Status\":\"Active\",\"SubChannels\":[],\"UnitOfMeasure\":null},{\"Description\":null,\"Id\":\"CH14\",\"IsGhost\":false,\"Name\":\"CH14\",\"Status\":\"Active\",\"SubChannels\":[],\"UnitOfMeasure\":null},{\"Description\":null,\"Id\":\"CH15\",\"IsGhost\":false,\"Name\":\"CH15\",\"Status\":\"Active\",\"SubChannels\":[],\"UnitOfMeasure\":null},{\"Description\":null,\"Id\":\"CH16\",\"IsGhost\":false,\"Name\":\"CH16\",\"Status\":\"Active\",\"SubChannels\":[],\"UnitOfMeasure\":null},{\"Description\":null,\"Id\":\"CH17\",\"IsGhost\":false,\"Name\":\"CH17\",\"Status\":\"Active\",\"SubChannels\":[],\"UnitOfMeasure\":null},{\"Description\":null,\"Id\":\"CH18\",\"IsGhost\":false,\"Name\":\"CH18\",\"Status\":\"Active\",\"SubChannels\":[],\"UnitOfMeasure\":null}],\"UnitOfMeasure\":null}],\"Commands\":[],\"DataInterval\":150,\"Id\":\"736C8F78-23A6-498B-9E00-04B8B73FCF1B\",\"IsGenerated\":true,\"Name\":\"Arduino Uno\",\"Version\":null,\"BaudRate\":9600}"]
["This manifest was generated for the connected device. You can edit the device name and channel data here and the Data In worksheet will be updated."]
[null,"Channels"]
[null,null,null,null,null,null,null,null,"Data Source Id"]
[null,null,"Id","Name","Description","Unit of Measure","Active",null,"736C8F78-23A6-498B-9E00-04B8B73FCF1B",null,1]
[null,null,"CH1","CH1",null,null,"ü",null,"Data Interval (ms)"]
[null,null,"CH2","CH2",null,null,"ü",null,150]
[null,null,"CH3","CH3",null,null,"ü",null,"Baud Rate"]
[null,null,"CH4","CH4",null,null,"ü",null,9600]
[null,null,"CH5","CH5",null,null,"ü"]
[null,null,"CH6","CH6",null,null,"ü"]
[null,null,"CH7","CH7",null,null,"ü"]
[null,null,"CH8","CH8",null,null,"ü"]
[null,null,"CH9","CH9",null,null,"ü"]
[null,null,"CH10","CH10",null,null,"ü"]
[null,null,"CH11","CH11",null,null,"ü"]
[null,null,"CH12","CH12",null,null,"ü"]
[null,null,"CH13","CH13",null,null,"ü"]
[null,null,"CH14","CH14",null,null,"ü"]
[null,null,"CH15","CH15",null,null,"ü"]
[null,null,"CH16","CH16",null,null,"ü"]
[null,null,"CH17","CH17",null,null,"ü"]
[null,null,"CH18","CH18",null,null,"ü"]